+========================================+
| Reversion Information for DCON Utility |
+========================================+
[Version 4.3.9] [September,8,2005]  
  New Support Modules:
    M87019,M87015,i-87019,i-87015 modbus and DCON protocol modules.
    M7024 Analog output module
    M7041,M7045,M7050,M7051,M7052,M7053,M7055,M87063,M87055,M87040,M87041,M87053 modbus DIO modules.
    M7015,M7033 modbus protocol modules

  Modify:
    7019 module add CJC adjustment for each channel.
    7018,87018 add CJC adjustment for each channel
    i-7015,i-7033,i-7013 support new type code 0x2E,0x2F,0x80,8x81.
    i-7021,i-7022 support new hex data format.
    7080 add new function to set the filter setting to default value.
    i-8000 MCU add new function to reverse the DI active status.
    
  Fixed Bug:
    debug 7019 when setting type code will show run time error.
    when modules' checksum are enabled,it will get the wrong firmware version.
    when thermocouple module's AI values are close to -0 ,it will get -0000 under range error code.
    i-7005 module can not link to Help file.
    
  Note1:The i-8000 DCON firmware must be A3.05 or above to support the DI active status reverse function.
       
       
[Version 4.3.8] [March,2,2005]  
  Fixed Bug:
    Install Shield package not include "MSWINSCK.OCX" and 
    wil get run time error, if Windows\system32\ does not have this file.

[Version 4.3.7] [February,1,2005]  
  New Support Modules:
    i-7045,i-7055 I/O modules
    M7067 Modbus RTU Protocol modules.
    7188EF-016 RFNet modules
    WinCon:when 87K module are plugged into WinCon I/O slots.
  Modify:
    Thermocouple module add CJC enable/disable function.
  Note:
    i7000.DLL must be ver 5.1.4 to support i-7045,i-7055,7188EF-016 FRNet.

[Version 4.3.6] [December,27,2004]  
  New Support Modules:
    i-7051 16 channel DI unit
    M7060,M7017,M7018,M7019 Modbus RTU Protocol modules.

  Modify:
    RunMonitor:
      1.support Modbus protocol
      2.add simple data log function

    8080 unit:
      Each channel can set channel mode independent

    7015 add type code 0x2E,0x2F,0x80,0x81
 
    7016 unit:
    2-Channel (By Switch):
      If 7016 firmware < B1.3
      It can not read two channels' value at a time.
      It needs to use command $AA0 or $AA1 to switch channel 
         and system need to delay 300 ms each time when program 
         use #AA to read each channel's value.
      In this case,the sampling rate is about 2 Hz.
	 
    2-Channel Mode:
      If 7016 firmware >= B1.3
      When program use command $AA332 to set 2-channel mode
        It can read two channels' values at a time by using #AA.
      In this case,the sampling rate is about 2 Hz.

    Single Channel:
      If 7016 firmware < B1.3
      It need to use command $AA30 or $AA31 to set to channel 0 or channel 1.
        then use command #AA to read the analog value.
      In this case,the sampling rate is about 10 Hz.
	
      If 7016 firmware >= B1.3
      It can use command $AA30 or $AA31 to set to channel 0 or channel 1.
        or use command $AA330 or $AA331 to set to channel 0 or channel 1.
        then use command #AA to read the analog value.
      In this case,the sampling rate is about 10 Hz.

  Fix Bug:
    87K Analog unit:
      87013,87017,87018 can not read AI value when address >=1
    Note :this bug will take place when these modules are plugged 
      in 87K I/O Expansion.
  Note:
    uart.dll must upgrade to 2.1.4 or above to support M7060,M7017,M7018,M7019 
    i7000.dll must upgrade to 5.1.3 or above to support i7051 and new 7016 command    
    firmware must upgrade to A3.0.3 to support new 8080 lib


[Version 4.3.5] [October,20,2004]  
  Fix Bug:
    8013(87K) when change SSTab page will get error description.
    When open 8024(87K) will get run time error.  

[Version 4.3.4] [October,7,2004]  
  Supported modules:
    7005 unviersal 8 channels thermistor with 6 Digital output module. 
  Modify: 
    7011,7012,7014,7016 units support power on value and safe value function.
    7011,7012,7014,7016,7033 support LED Display function.
    Add Version information at main form.

[Version 4.3.3] [August,5,2004]  
  New support modules:
    8050

  Note:
    DCON Firmware must be A3.0.1 to support 8050      
    I7000.DLL must be Ver 5.1.2    
    Uart.DLL has been upgraded to 2.1.1 


[Version 4.3.2] [Jun,15,2004]
  New support modules:
    7015
    8080 (*)
    (plugged into an I-8000 main control unit)
    87082	
     (plugged into an I-87K expansion unit)  

  Modify:
    1. 7019R write channel status(Enable/Disable) into EEPROM 
         when click check box.
    2. 8017H Get rid of filter rejection and data format setting (**)   
    3. Disable Slew rate setting of 8024 (**) 
  
  Fix bug:     
    1. 8017H can not set alarm to DO module that is plugged in slot4 ~ slot7
    2. 7012 can not apply alarm setting function.
    3. 7012 DI signal picture can not match the right value.
    4. 7014D linear mapping range display can not work properly.
    5. Utility can not run on Windows NT4.0.

  Note:
    *    for 8080, the firmware version must be A3.00 or above 
    **   for hardware does not support this function.

===========================Relative Information============================
Firmware
  For RS232,RS485
    CD:\NAPDOS\8000\841x881x\firmware
  For Ethernet
    CD:\NAPDOS\8000\843x883x\TCP\Vxcomm\Server(843x883x)
    
MiniOs7 image (40MHz):
  for 40MHz CPU ===> 8k040330.IMG 
    CD:\NAPDOS\8000\843x883x\TCP\Vxcomm\Server(843x883x)\os_image\40MHz
            
  for 80MHz CPU ===> 8e040420.IMG 
    CD:\NAPDOS\8000\843x883x\TCP\Vxcomm\Server(843x883x)\os_image\80MHz
 


[Version 4.3.1] [May,13,2004]
  Fix bug:
    1. 7019R when setting input range shows run time error 9.
    2. 87018 when adjust cjc offset up down shows  run time error 340.

  Update:
    1. firmware must be version A1.98 or above
    2. dll must be be version 5.0.9 or above
    3. uart.dll must be 2.0.5 or above

[Version 4.3.0] [Apr,22,2004]
  New support modules:
    7019
    87040,87041	
     (plugged into an I-8000 MCU or I-87K expansion unit)
	  		  	        
  Add new function:     
    1. All thermocouple modules can display cjc temperature and can adjust cjc offset
       include module 7011,7018,7019 and 
       87018 (plugged into an I-8000 MCU or I-87K expansion unit)
    2. all 87k digital input DI count\latch function has 
       been supported when these modules were plugged into 8K MCU.
 
  Modify:
   1. When 87k modules are plugged into the 8k MCU,
      the module's name will change to 80xx(87K).     

  Fix bug:
   1. 8017H input range was wrongly defined .
      Run Data log shows garbage sometimes.

  Update:
   1. firmware must be version A1.97 or above
   2. dll must be be version 5.0.9 or above
   3. uart.dll must be 2.0.5 or above

[Version 4.2.9] [Feb. 20,2004]
  Supported modules:
    8069, 87069
    (plugged into an I-8000 MCU or I-87K expansion unit)
  Fixed bugs:	        
    Run Data Logger unit:
  The generated log file can not be displayed normally 
    on the English Microsoft Platform		  	
    8017,8018 unit:
      DO Map Enable/Disable function mismatch 
      at the High Alarm Setting between channel 1 and channel 7.
  Modified:
    87K Digital I/O user interface:
      1. Combine frm8KDIO and frm87KDIO as frmDIO.
    87K digital input DI count\latch user interface:
      1. Completely resigned user interface
      2. Increase the support for max channel from 16 to 32 channels
    8017,8018 unit: 
      Added message box when setting the high alarm 
      and low alarm configuration of the 8017,8018 units.
    		
  Added new functions: 
    Terminal->Single Line:
      1. Timeout value can be adjusted.
      2. 8 set command line lists can be memorized.

    Note:
    I-8000 MCU Firmware must be version A1.96 or above to support 8069,87069.    


[Version 4.2.8] [Jan,05,2004]
  Fix bug:
    Setting module address error. Modules Address up down button 
    does not work, includes:
    7011,7011P,7012,7012F,7013,7014,
    7017C,7017FC,7017RC,7017R,7017FR,7017FRC,
    7018,7018P 
  Update:
    uart.dll  ===> 2.0.5
    7000.dll  ===> 5.0.9
    ICPCON.HLP is replaced by DCON_HELP.chm ver 1.0
  Add:
    add a module list that the Utility support.
    
    
[Version 4.2.7] [Oct,14,2003]
  Support modules:
    7017C,7017FC,7017RC,7017R,7017FR,7017FRC,
    7018BL,
    7058,
    8037
    
  Modify data logger:
    Log_Config.txt (original default.log) ===> to configure how to log data
    Log_Report.txt (original report.log)  ===> the logged data
    The syntax is also chnaged.
    Please refer to the comment in the Log_Config.txt.
    
  Fix bug:
    Setting 87017 in 87K expansion unit error.
             
Update:
  uart.dll  ===> 2.0.4
  i7000.dll ===> 5.0.8
  Note: Firmware of I-8000 MCU must be A1.95 to support 8037.

[Version 4.2.6] [Jun,13,2003]
  Remove files:
    Dones't copy following files to windows\system.
    mfc42.dll, msvcrt.dll, msvcrt20.dll, 
    oledlg.dll, riched32.dll
            
  Change directory:
    Copies following files to DCON_Utility directory 
    instead of windows\system.
    olepro32.dll, oleaut32.dll, stdole2.dll, 
    asycfilt.dll, msvbvm60.dll
            
Fix bug:
  Cannot recognize the difference between 7018 and 7018P.

[Version 4.2.5] [Apr,25,2003]
  Update: 
    i7000.dll ==> 5.0.6
        
  Support:
    1. 87022 (plugged in I-87K expansion unit)
    2. 87026 (plugged in I-8000 MCU or I-87K expansion unit)
    (command sets are same as 87022)
		
    Note: Firmware of I-8000 MCU must be A1.94

[Version 4.2.4] [Jan,16,2003]
  Change name of the Utility to DCON Utility
    
  Update: 
    i7000.dll ==> 5.0.5
  Support:
    1. 8077 (command sets are same as 8054)
    2. 8017MP (command sets are same as 8017H)
    3. 8017LP (command sets are same as 8017H)
    4. 87022 (plugged in I-8000 MCU)
    (command sets are same as 87024 plugged in I-8000 MCU)
		
  Note: 
    1. MiniOS7 must update to 1.04 build 012, Dec, 27, 2002
    2. Firmware of I-8000 MCU must be A1.93
		
[Version 4.2.3] [Nov,05,2002]
  Fix:
    87018 input range support 3 T/C type
      1. L-type
      2. M-type
      3. L-type(DIN43710)
  Note:
    Firmware of I-8000 MCU must update to version A1.91 or later.
		
[Version 4.2.2] [Oct,29,2002]
  Fix:
    [Run-time error: 13] 
      when click 87017 that plug on 87K expansion unit.
	
[Version 4.2.1] [Oct,15,2002]
  Fix:
    [Run-time error: 339] 
      when click 8K digital mudules that plug on I-8000 MCU.

[Version 4.2.0] [Sep,24,2002]
  Update: 
    i7000.dll ==> 5.0.3
  Support:
    8040,8041,8042
  Add:
    Power On Value, Safe Value setting of 8k DO, DIO modules
		
[Version 4.1.2] [Jul,11,2002]
  Update:
    uart.dll  ==> 2.0.1	
    i7000.dll ==> 5.0.2 
  Add:
    Excitation voltage configuration for 7016
					
[Version 4.1.1] [Apr,3,2002]
  Add:
    Fast Mode for 87017
    Filter Setting for 87013
    87017
    87018	

[Version 4.1.0] [Mar,17,2002]
  Update:
    uart.dll  ==> 2.0.0	
    i7000.dll ==> 5.0.0		
  Fix:
    8013,87013 reads values error.	

[Version 4.0.9] [Feb,29,2002]
  Support 8058, 87058
  Fix:
    Checks the COM port before searching.

[Version 4.0.8] [Jan,22,2002]
  Fix:
    1. searching error when address >= 16(Dec).
    2. setting 8017 & 87017 error when address >= 16(Dec).

[Version 4.0.7] [Jan,14,2002]
  Upgrade	uart.dll   14-Jan-2002 pm 1:39   8.13 Sleep version
    to reduce CPU resource consumption.
	
[Version 4.0.4 Beta2] [Nov,19,2001]
  Support 752N
    Search 8X3X/8X4X by only one address (skip N-1 address).

[Version 4.0.4] [Oct,20,2001] by Kevin
  Fix:
    1. Run log file, first line is explain.
      For example: "This is test log."
    2. Search timeout is too short.
       
  Support 8X3X, 8X4X. 
  Search 8X3X/8X4X by only one baudrate.

[Version 4.0.3] [Oct,190,2001] by Kevin
  Remove auto search function
      
[Version 4.0.2]
  i7000.dll  10-July-2001 pm 3:14   0460  
  uart.dll   13-July-2001 pm 5:43   8.1
   
  fix: 
    1. 8017 T/C input range mapping error
    2. 8017 Filter selection error

  change:
    1. Timeout of open comport change to be 2 seconds 
      ( original timeout is 10 seconds)
    2. Install i7000.dll and uart.dll into 7000 Utility directory 
      ( original into windows\system)

+============+
| Files List |
+============+

Below files will be installed into c:\DAQPro\DCON_Utility

DCON_Utility.exe
icpcon.cfg
icpcon.hlp
default.log

i7000.dll
uart.dll
Knob.ocx
NumLed.ocx
Odemeter.ocx
Selector.ocx
Toggle.ocx

Misc06.ico
Misc15.ico
No2.ico
Off2.ico
On2.ico		