/****************************************************************************/
/* A822/A8112 DLL Driver and OCX(ActiveX) Control 		                      */
/* for Windows NT                                                 */
/*                                                             	    		    */
/* Version : 3.2.1                                    		                  */
/* Update  : Apr-18-2006                          		                      */
/*                                                                  		    */
/* Support : A822 PGH/PGL, A8112 DG/HG                                      */
/*                                                                          */
/****************************************************************************/

A. The default installation folder is 
   C:\DAQPro\A822_WinNT
      
B. It's recommended to install the software before plug PIO-DIO series cards
   into the computer. This reduces the Windows Plug & Play procedures.
     
     1. Run the setup program to install.
     2. Power-off your computer.
     3. Plug the A822/A8112 series cards into the computer.
     4. Re-start the computer and finish the Windows PnP.
     
   Usually, Windows 2000 will finish the PnP procedures automatically.
   If Windows still asking the Inf files for PnP, please specify the
   "C:\DAQPro\A822_Win2K\Driver" (depends on your installation) 
   folder to finish it.

C. For more information please refer to:
   
   CD:\NAPDOS\ISA\A822\Manual           (Hardware manual)
   CD:\NAPDOS\ISA\A822\DLL_OCX\Demo     (Sample programs)
   CD:\NAPDOS\ISA\Manual                (Related documents)

Note: It will return A822_DriverOpenError under Windows 2000 when the 
      driver found no devices on the system.



Note: The manual is written in PDF format, users may need to free 
      download the Adobe Arcobat Reader at
      http://www.adobe.com/prodindex/acrobat/readstep.html
      or
      CD:\NAPDOS\Adobe_Reader
