*****************************
Feb-20-2004

New Release
    
*****************************
[Ver 1.17 2008-01-15]
    1. Support PCM-CAN200
    2. Support PISO-CAN200U\PISO-CAN200E\PISO-CAN400U\PISO-CAN400E
    3. CAN Utility V3.02
[Ver 1.16 2007-07-09]
    1. Add RemoveIrq() function into CloseBoard() function
    2. Add new function CAN_ConfigWithoutStruct(...)" for some development that can't use structure
    3. Fix the CAN Utility bug which cause the utility crash when load a configure file
[Ver 1.15 2007-03-02]
    1. Fix CAN_SendMsg( ) 29-bits ID critical section bug
    2. Add new function "CAN_SendWithoutStruct(...)" for some development that can't use structure
    3. Add new function "CAN_ReceiveWithoutStruct(...)" for some development that can't use structure
[Ver 1.14 2006-07-30]
    1. Fix CAN_ReceiveMsg() critical section bug
    2. Fix the bug of memery error in  the KP_CAN.sys
    3. Modify the bug in interrupt function in the KP_CAN.sys
    4. Add new function "CAN_GetCardPortNum()" to get port number of a CAN card before active board
[Ver 1.13 2005-06-30]
    1. Fix the Utility tool bug which cause the sheet title disappeared
    2. Put the msvbvm60.dll in the local folder to avoid error when install the driver
    3. Fix the buf of CAN_Init() function in the pisocan.dll file.
[Ver 1.12 2004-12-24]
    1. Solve the conflect with PISO-CM100
    2. Solve the problem about the capture of IRQ resource when release the dll resource
    3. Modify the bug of function Clear CAN_ClearSoftBuffer and CAN_ClearDataOverrun
[Ver 1.11 2004-11-22]
    1. Modify the bug of sending the extend CAN messages.
    2. Add the judgement parameters of the memory allocation.
[Ver 1.10 2004-09-17]
    1. Add MsgTimeStamps parameters for reception CAN messages.
    2. Modify the resource free function.
    3. Compact the dll source code.
    4. Fix the bug about to active the inexistent board.
    5. Keep the last CAN message in the last record of software buffer when buffer overruns.

[Ver 1.01 2004-06-17]
    1. Enhance performance
    2. Solve the problem of receive data lose
    3. Use different sub-device ID to distinguish PISO-CAN200 and PISO-CAN400
    4. Solve the proglem of DLL share
    5. Fix the bug of  the DEMO, Utility, and Manual
    6. Use 3K buffer for one CAN Port