/*****************************************************************************/
/*                                                                           */
/* PISOCAN DASYLab CAN Driver                                                */
/* for Windows 2000/XP	                                                     */
/*                                                                           */
/* Version : 1.0                                                             */
/* Update  : 2006/04/25                                                      */
/*                                                                           */
/* Support : PISO-CAN200/400                                                 */
/*                                                                           */
/*                                                                           */
/*****************************************************************************/
/*               This content is valid only for WINDOWS 2000/XP              */
/*****************************************************************************/


 A). The Disk Contents:

  |--\README.TXT             	 <-- this file
  |--\WhatNew.TXT
  |--\DASYLab_CAN.EXE         	 <-- the Setup program    
  |--\DASYLabCAN.pdf   	      	 <---user manual
  |--\DASYLabCAN_QuickStart.pdf  <---quick Start
     
      
 B). Installation Steps
    step 1). Install the PISO-CAN200/400 driver(H:\CAN\PCI\PISO-CAN200/400)(if CD-ROM drive is H:)
    step 2). Install the DASYLab CAN driver
             The setup path as:(if CD-ROM drive is H:)
             H:\CAN\PCI\PISO-CAN200/400\DASYLab_CAN_driver\
    step 3). Following those instructions in installation process 
             to complete it.



 C). After finishing the installation,

     The DASYLab CAN Library will be copied into C:\DAQPro\PISO-CAN\DASYLab_CAN\Dirver\
     The Manual will be copied into C:\DAQPro\PISO-CAN\DASYLab_CAN\Manual
     The Demo programs will be copied into C:\DAQPro\PISO-CAN\DASYLab_CAN\Demo
     

 D). After installed, the sub-directory tree as follows:

     The default [Base Directory] is "\DAQPro\PISO-CAN\DASYLab_CAN".

   [Base Directory] <-- the directory you selected to setup
    |
    |
    |--\Demo                           <-- Demo Programs
    |	|--\Demo1.dsb			  <-- Demo 1
    |	|--\Demo2.dsb			  <-- Demo 2
    |   |         
    |	|
    |--\Driver                         <-- some device driver
    |	|--\DlIcCAN.DLL			  <-- Dll file of DASYLab CAN driver			
    |
    |--\Manual
    |   |--\DASYLabCAN.pdf             <-- DASYLab CAN driver user's manual 
    |   |--\DASYLabCAN_QuickStart.pdf  <-- DASYLab CAN driver quick Start 
    |
    |--\WhatNew.TXT                    <-- What's New.
    |--\README.TXT                     <-- this file.



 E). After installed, the following links will be add into the "Start Menu".
    
   [Start]    <-- the Start menu
    +--\Programs
        +--\DAQPro     
            +--\PISO-CAN           
                +--\DASYLab_CAN     <-- link to the "DASYLab_CAN" folder


Note: The PCI/PIO/PISO Series Cards must set  it's  Information-file (.INF file) 
          correctly under Windows 98/Me/2000/XP before controling (accessing) 
          these cards. For the detail informations, please refer to 
          PISO-CAN\Manual\PnPInstall.PDF.

Note: These manuals are PDF format. In order to view these manuals, users can 
          free download the Adobe Arcobat Reader and install it at
          http://www.adobe.com/prodindex/acrobat/readstep.html
