2013/07/2 by Andy
Utility:  1. v3.1.0 to v3.1.1
	  2. fix bug of F-8084 that use wrong Modbus address

----------------------------------------------------------------------

2013/07/15 by Andy

firmware: 1. v3.00 to v3.01
	  2. suppport F-8019, F-8028CV

Utility:  1. v3.00 to v3.1.0
	  2. suppport F-8019, F-8028CV

----------------------------------------------------------------------

2013/06/07 by Andy

firmware: 1. v2.00 to v3.00
	  2. modify IOM ID
	  3. modify PO, PI IOM function
	  4. modify channel break EMCY function
	  5. modify MCU Status Address & Common IOM Address Modbus Address
	  6. suppport F-8040, F-8041

Utility:  1. v2.00 to v3.00
	  2. modify MCU Status Address & Common IOM Address Modbus Address
	  3. modify PO, PI IOM function
	  4. modify channel break EMCY function
	  5. suppport F-8040, F-8041

----------------------------------------------------------------------

2011/11/17 by Andy

firmware: 1. v1.02 to v2.00
	  2. hardware update; firmware change hardware power register and connector pin
	  3. add port 10000 command for reading firwmare version
	  4. modify read/write modbus_configuration_command
	  5. add CAOI-03 and CAOI-04 IOM

Utility:  1. v1.02 to v2.00
	  2. add port 10000 command for reading firwmare version
	  3. modify read/write modbus_configuration_command

----------------------------------------------------------------------
2011/03/03 by Andy

firmware: 1. v1.01 to v1.02
	  2. Modify specific Modbus Read configuration command from 
             base 0x1000 to 0x8000
 	  3. Add Modbus address for HART command:
	     Write HART command => AO address: 256 ~ 512
	     Read HART command => AI address: 5120 ~ 7168

Utility:  1. v1.01 to v1.02
	  2. Modify specific Modbus Read configuration command from 
             base 0x1000 to 0x8000
	  3. Add HART command test function

----------------------------------------------------------------------
2010/06/18 by Andy

firmware: 1. v1.00 to v1.01
	  2. Add F-8041P PO IOM
	  3. Modify Individual IOM Modbus memory
	     1024 ~ 1535 => Slot0, 1536 ~ 2047 => Slot1 .... 

Utility:  1. v1.00 to v1.01
	  2. Add F-8041P PO IOM
	  3. fix error Modbus Memory for PI IOM