I7000DLL

[Date2006/07/27][Ver 5.18] by martin
  Modify:
  DigitalIOReadBackGroup_FR     
  DigitalIOReadBackBit_FR  
  DigitalOnLineStatus_FR
  parameter wType=0 Read Group DO Value, wType=1 Read Group DI Value
  Note1: The definition of wType changed in firmware 1.0.06 of 7188EF-016.
  Note2: There is no change in dll source code, but the definition of wType changed in firmware.
  So the applications must change the parameter wType if they have included the above functions.
----------------------------------------------------------------------------------------------------------

[Date2006/04/25][Ver 5.17] by martin
DLL released: 25-April-2006
  New Support for i-8017HS 16 channel AI
  use old function:
    AnalogIn_8K
    
  New Support for i-8082 Frequency module
  new function:
    FloatFreq_All_8K
    FloatFreq_8K
  New Support for i-8046
  use old function:
    DigitalIn_8K
  New Support for i-87015,i-87019 AI module on i-8000 system
  use old function:
    AnalogIn_8K
    AnalogInFsr_8K
    AnalogInHex_8K
    AnalogInAll_8K
    SetAlarmConnect_8K
    ReadAlarmMode_8K
    SetAlarmLimitValue_8K
    ReadAlarmLimitValue_8K
    ClearLatchAlarm_8K
    SetAlarmMode_8K
    ReadAlarmStatus_8K
  New Support for i-87082 Counter/Frequency module on i-8000 system
    ReadCounter
    ReadFreq
    ClearCounter
    SetCounterStatus
    ReadCounterStatus
  Note i-8082 and i-87082 are totally different module and use different functions,
  although they use the same ID 0x8282 in i7000.dll
----------------------------------------------------------------------------------------------------------


[Date:2005/10/17][Ver 5.16] by martin
DLL released: 04-Oct-2005

  New Support for i-87015,i-87019 AI module
  use old functions ==>
   	AnalogIn_All_87K
 	AnalogIn_87K

  Debug:
	SetAlarmLimitValue 
	  when type code =0x0E (J Type), the wPoints=2 not 3
	AnalogIn_All
	  when the AI values are rear -0000.0, will return under range error code.
	ReadCounter
	  when the couter values are in hex format,there are bugs for string processing. 
----------------------------------------------------------------------------------------------------------
[Date:2005/05/06][Ver 5.1.5] by martin
Module: 7188EF-016
  new function:
	DigitalOutAll_FR						 
	DigitalOutGroup_FR						 
	DigitalOutBit_FR						 
	DigitalIOReadBackAll_FR					 
	DigitalIOReadBackGroup_FR				 
	DigitalIOReadBackBit_FR					 
	DigitalOnLineStatus_FR					 
	GetChCount_FR	  				
			    

Module: 8080
  new function:
    ReadUpDownDirPulse_All  (support signed long data type)	
	ReadUpDownDirPulse	    (support signed long data type)				 
  Modify:
	ReadCounter		        (support unsigned long data type)					     	
	ReadCounter_All		    (support unsigned long data type)					 
	ReadFreq                (support unsigned long data type)
  Note: DCON firmware E10M_nnn.exe and DCON_nnn.exe must be A3.05 or above to support 
        the modified command format.
        
Module: 7045       		
use old functions ==>
    SetSafeValueForDo
    ReadSafeValueForDo
    SetPowerOnValueForDo
    ReadPowerOnValueForDo
    DigitalOut
    DigitalBitOut
    DigitalOutReadBack
    
    
Module: 7055
use old functions ==>
    SetSafeValueForDo
    ReadSafeValueForDo
    SetPowerOnValueForDo
    ReadPowerOnValueForDo
    DigitalOut
    DigitalBitOut
    DigitalOutReadBack
    DigitalIn
    DigitalInCounterRead
    ClearDigitalInCounter
    DigitalInLatch
    ClearDigitalInLatch
----------------------------------------------------------------------------------------------------------


[Date:2004/8/5][Ver 5.1.2] by martin
Debug:
  readCounter readMode=2 dwBuf[9]==>counter or frequency value
    dwBuf[10]==>overflow value

----------------------------------------------------------------------------------------------------------
[Date:2004/7/20][Ver 5.1.1] by martin

Module: 7080 *(Note 1) ,87082,8080 
use new functions ==>
ReadCounter,ReadCounter_All,ReadFreq,ReadFreq_All,
	ClearCounter,SetCounterStatus,ReadCounterStatus

Note1: User can choose original 7080 series functions or these new functions

Module: All 87K *(Note 2) DI and DIO modules when plugged into 8K MCU
use new functions ==>
DigitalIn_8K, DigitalInCounterRead_8K, 
	ClearDigitalInCounter_8K, DigitalInLatch_8K

Note2: All 87K I/O modules when plugged into 8K MCU look as 8K
	dwBuf[2] => module ID 
	must be : 0x8051/0x8052/0x8053/0x8054/0x8055/0x8058/0x8063/0x8040
	not : 0x87051/0x87052/0x87053/0x87054/0x87055/0x87058/0x87063/0x87040

Module: 7019 
use old functions ==>
AnalogIn,AnalogInFsr,AnalogInHex,AnalogIn8,AnalogInAll

Module: 7015 
use old functions ==>
AnalogIn,AnalogInFsr,AnalogInHex,AnalogInAll

Module: 87040 
use old functions ==>
DigitalIn_87K, DigitalInCounterRead_87K, 
	ClearDigitalInCounter_87K, DigitalInLatch_87K

Module: 87041 
use old functions ==>
DigitalOut_87K,DigitalBitOut_87K,DigitalOutReadBack_87K

Module: 8050 
use old functions ==>
DigitalBitOut_8K,DigitalOut_8K,DigitalIn_8K,DigitalOutReadBack_8K

Module: 8069
use old functions ==>
DigitalOut_8K,DigitalBitOut_8K,DigitalOutReadBack_8K 
 
Modify:
	1.AnalogIn for 7016 can set parameter to selecte channel to read Analog data

Update:Uart.DLL ==>2.1.1
----------------------------------------------------------------------------------------------------------
[Date:2003/9/10][Ver 5.0.8] by Sean
Add:
	1. DigitalOut_8K supports, DigitalBitOut_8K, DigitalOutReadBack_8K
	support to I8037
	2. DigitalIn, DigitalInCounterRead, ClearDigitalInCounter
	support to I7058
Modify:
	Modify the all souce code for Microsoft Windows OS and WinCE OS
Update:Uart.DLL ==>2.0.4
----------------------------------------------------------------------------------------------------------
[Date:2003/6/12][Ver 5.0.7] by Sean
Fix bug:
	AnalogOutHex
	AnalogOutFsr
Modify:
	AnalogInAll
	AnalogInAll_87K
Update:Uart.DLL ==>2.0.3
----------------------------------------------------------------------------------------------------------
[Date:][Ver 5.0.6] by Sean
Modify:
	1.wrong:
		if(strlen(szRec8k)==7)
	correct:
		if(strlen(szRec8k)==6)
		AnalogIn(),AnalogInHex(),AnalogInFsr()
		AnalogIn_8K(),AnalogInHex_8K(),AnalogInFsr_8K()
		AnalogIn_87K(),AnalogInHex_87K(),AnalogInFsr_87K()[03/03/10]
	2.Modify 4 parameter name in all functions of I7000.c['03/05/05]
	3.AnalogInHex_8K dwBuf[7] --->dwBuf[8]['03/05/05]

Fix bug:
	AnalogOutReadBackHex
Add: 
	AnalogOutHex_87K support to I87022/87026
	AnalogOutFsr_87K support to I87022/87026 
	AnalogOutReadBackHex_87K[03/04/24]
	AnalogOutReadBackFsr
	AnalogOutReadBackFsr_87K[03/04/25]


Update:Uart.DLL ==>2.0.2
-----------------------------------------------------------------------------------------------------------------
[Ver 5.0.5] by Sean

	Modify:	1.i7000.c  [2002/11/20][2003/01/08]	
		AnalogIn8()

		2.i87000.c	[2003/01/06]
		DigitalOut_87K

	Fix bug:1.i8000.c,i87000.c	[2002/11/06]
		AnalogInFsr_8K,AnalogInHex_8K,AnalogInFsr_87K,AnalogInHex_87K		

		2.i8000.c [2003/01/02]
		ReadAlarmStatus_8K,ReadAlarmMode_8K,ClearLatchAlarm_8K
		SetAlarmMode_8K,ReadAlarmStatus_8K,SetConfigurationStatus_8K,
		ReadConfigurationStatus_8K,SetStartUpValue_8K,ReadStartUpValue_8K

		3.i87000.c [2003/01/02]
		SetStartUpValue_87K,ReadStartUpValue_87K		

		4.i7000.c	[2003/01/20]
		SetConfiguration_7080
		Send command 'szCmd',lowcase change as uppercase 

		5.ReadSafeValueForAo()
		  if(wCheckSum==0) wRecStrLen=10; else wRecStrLen=12;
		  modified as
		  if(wCheckSum==0) wRecStrLen=9; else wRecStrLen=11;//for 7021/7021P/7022
		6.AnalogInAll  [2003/03/28]
		7.AnalogInAll_87K[2003/03/28]

	ADD:  1.DigitalOut_8K(),DigitalBitOut_8K(),DigitalIn_8K() support to 
	      module I-8077[2003/01/22]
	      2.SetSafeValueForDo(),SetPowerOnValueForDo(),
		ReadPowerOnValueForDo(),ReadSafeValueForDo()
	      support to module I-7063/63D/63A/63AD/63B/63BD and I-7066/66D
	      3.DigitalOutReadBack(),DigitalBitOut() support to module I-7066/66D
	Delete:SetConfigurationStatus_8K(),SetConfigurationStatus_87K()

	Update:Uart.DLL ==>2.0.2
-----------------------------------------------------------------------------------------------------------------
[Date: 10,22,2002] [Ver 5.0.4] by Sean
	Add:1.add the function AnalogOutHex for I7021/21p/22
	Add:2.add the function AnalogOutFsr for I7021/21p/22
	Add:3.add the function AnalogOutHexReadback for I7021/21p/22

[Date: Sept,20,2002] [Ver 5.0.3] by Sean
	Add:1.add the modules 8058,8040,8042 to DigitalIn_8K
	    2.add the modules 8041,8042 to DigitalBitOut_8K,DigitalOut_8K,DigitalOutReadBack_8K
	    3.add the modules 87058 to DigitalIn_87K
	Modify:1. modify return of DigitalIn_8K(),DigitalOutReadBack_8K()
		  ex:  sscanf(szRec8K,"!AA%04X",&dwBuf[5]);
	       2. HostIsOK() function change Send_Receive_Cmd() to Send_Cmd()
		  because ~**,no response
----------------------------------------------------------------------------------------------------------
[Date: July,11,2002] [Ver 5.0.2] by Sean
	Add:1.ReadConfigStatus to i7000.def
            2.AnalogInFsr_87K,AnalogInHex_87K,ReadStartUpValue_87K,SetConfigurationStatus_87K
              SetStartUpValue_87K to i8700.h
	    3.AnalogInFsr_8K,AnalogInHex_8K,SetConfigurationStatus_8K,MakeCRC16Table
              to i8000.h
        Remove:SetPowerOnAndSafeValue from dll
	Modify:WORD CALLBACK Get_Dll_Version(void)
	{
		return(0x502);	(DEC changed as Hex)
	}
	Update:Uart.DLL ==>2.0.1
----------------------------------------------------------------------------------------------------------	
[Date: Apr,15,2002]  [Ver 5.0.1] by Kevin
	Modify AnalogIn8, AnalogInAll_8K, AnalogInAll_87K
----------------------------------------------------------------------------------------------------------
[Date: Mar,19,2002]  [Ver 5.0.0] by Kevin
	Add:    AnalgoIn_87K to i8700.h
	Fix:    87013 reads values error.
	Modify: Declaration of export/import functions
	Remove: 1. DigitalOut, DigitalIn from i87000.h 
		2. Test, Float_Sub_2, Short_Sub_2 from i7000.h and i7000.c
	Update: Uart.Dll ==> 2.0.0	
----------------------------------------------------------------------------------------------------------	
[Date: Jan-19, 2000]  [Ver 4.20]
  1. Modify following function
        DigitalOut(......)
----------------------------------------------------------------------------------------------------------
[Date: Dec-9, 1999]   [Ver 4.10]
  1.  Modify following function
        AnalogOut(......) that supports 7022
        AnalogOutReadBack(......) that supports 7022
        ReadEventCounter(......) fix a bug that is when checksum enable, the event count value is wrong
        SetPowerOnValueForAo(......) that supports 7022
        SetSafeValueForAo(......) that supports 7022
  2.  added follow function
        ReadSafeValueForAo(......) that supports 7021/7022/7024 
        ReadPowerOnValueForAo(......) that supports 7024
----------------------------------------------------------------------------------------------------------
[Date: Aug-24, 1999]   [Ver 4.00]
  1.  updated from [Ver 0350-255]
  2.  Modify following function
        DigitalIn(......) that support 7063 and 7065
  3.  added following function
        DigitalBitOut(......) for Digital Output Module
        ReadPowerOnValueForDo(......)
        ReadSafeValueForDo(......)
        DigitalInCounterRead(......)   
        ClearDigitalInCounter(.......)
----------------------------------------------------------------------------------------------------------
[Date: July-15, 1999]  [Ver 0350-255]
  1.  [Ver 3.50] with support 255 COM Ports

----------------------------------------------------------------------------------------------------------
[Date: June-16, 1999]  [Ver 3.50]
  1.  AnalogIn(......), AnalogInFsr(......), AnalogInHex(......) support 7016
  2.  AnalogOut(......) support 7016
  3.  ReadEventCounter(......) support 7016
  4.  SetAlarmLimitValue(......) support 7016
  5.  ClearLatchAlarm(......) support 7016
  6.  ReadOutputAlarmState(......) support 7016
  7.  DigitalIn(......) support 7016
  8.  EnableAlarm(......), DisableAlarm(......) support 7016 
  9.  SetPowerOnValueForDo(...)   fix the bug for 7060
  10. SetSafeValueForDo(...)      fix the bug for 7060
  11. Added following function:
         SetLedDisplay(......)  support 7016/7033  
         SetupLinearMapping(......) support 7014/7016
         EnableLinearMapping(......) support 7014/7016
         DisableLinearMapping(......) support 7014/7016
         ReadLinearMappingStatus(......) support 7014/7016
         DigitalOut_7016(......) support 7016
----------------------------------------------------------------------------------------------------------
[Date:  May-20, 1999]  [Ver 3.40]
  1. AnalogIn(......), AnalogInFsr(......), AnalogInHex(......) support 7033
  2. Added following function
        SetLedDisplay_7033(.....)
        GetLedDisplay_7033(.....)	
----------------------------------------------------------------------------------------------------------
[Date:  Mar-12, 1999]  [Ver 3.30]
  AnalogIn()

     if( (w7000[2]!=0x7013 && w7000[2]!=0x7011 && w7000[2]!=0x7018 ) && (strlen(szRec)!=wRecStrLen) )
     {
        err=ResultStrCheckError;
        goto ret_err;
     }

     //-----  Added by Shu, 7011, 7013, 7018
     if( w7000[2]==0x7013 || w7000[2]==0x7011 || w7000[2]==0x7018 )
     {
	 if( !memcmp(szRec,">-0000",6) )
	 {
	     err=UnderInputRange;
	     goto ret_err;
	 }
	 if( !memcmp(szRec,">+9999",6) )
	 {
	     err=ExceedInputRange;
	     goto ret_err;
	 }
     }

----------------------------------------------------------------------------------------------------------
[Date:	Jan-14, 1999]  [Ver 3.30]
  A. *** replace the UART.DLL and UART.LIB with new version
  B. *** Add the following function
       SetSafeValue()
       ReadSaveValue()
       SetPowerOnAndSafeValue()

/*----- 7011/7012/7014 Set Power On and Safe value ---------*/
EXPORTS WORD CALLBACK SetPowerOnAndSafeValue(WORD w7000[], float f7000[],
	char szSendTo7000[], char szReceiveFrom7000[]);
//---------------------- input -------------------------------------
//w7000[0];   // RS-232 port number: 1/2/3/4
//w7000[1];   // module address: 0x00 to 0xFF
//w7000[2];   // module ID: 0x7011
//w7000[3];   // checksum: 0=disable, 1=enable
//w7000[4];   // TimeOut constant: normal=100  , 0.1 second
//w7000[5];   // 0xPPSS:  PP=Power On value   SS=safe value
	      //	      00: DO0 -> Off   DO1 -> Off
	      //	      01: DO0 -> On    DO1 -> Off
	      //	      02: DO0 -> Off   DO1 -> On
	      //	      03: DO0 -> On    DO1 -> On
//w7000[6];   // flag: 0=no save, 1=save send/receive string
----------------------------------------------------------------------------------------------------------
[Date:	OCT-26, 1998]  [Ver 3.20]
    *** Modifying some functions for 7024.
		AnalogOut(), AnalogOutReadBack()
    *** Adding SetConfiguration_7080() function
	/************************************************************/
	/**************** modified function  ************************/
	/************************************************************/
	EXPORTS WORD CALLBACK AnalogOut(WORD w7000[], float f7000[],
		char szSendTo7000[], char szReceiveFrom7000[])
	{
	  char	  wPort,wFlag,c1,c2;
	  WORD	  wAddr,wRetVal,i,wID,wCheckSum,wTimeOut,err,wT,wChannel;
	  float   fVal;
	  WORD	  wRecStrLen;
	  char	  OutCh[10];

	  //---------------------- input -------------------------------------
	  wPort=(char)w7000[0];   // RS-232 port number: 1/2/3/4
	  wAddr=w7000[1];	  // module address: 0x00 to 0xFF
	  wID=w7000[2]; 	  // module ID: 0x7021
	  wCheckSum=w7000[3];	  // checksum: 0=disable, 1=enable
	  wTimeOut=w7000[4];	  // TimeOut constant: normal=100
	  wChannel=w7000[5];	  // Not used if module ID is 7021
				  // Channel No.(0 to 3) if module ID is 7024
	  wFlag=(char)w7000[6];   // flag: 0=no save, 1=save send/receive string
	  fVal=f7000[0];	  // DA output value: from 0.0 to 10.0
	  //---------------------- output ------------------------------------
				  // void

	/************************************************************/
	/**************** modified function  ************************/
	/************************************************************/
	EXPORTS WORD CALLBACK AnalogOutReadBack(WORD w7000[], float f7000[],
		char szSendTo7000[], char szReceiveFrom7000[])
	{
	   char  wPort,wFlag,cc[80],c1,c2;
	   WORD  wAddr,wRetVal,i,j,wReadType,wID,wCheckSum,err,wT,wTimeOut,wChannel;
	   WORD  wRecStrLen;

	   //---------------------- input -------------------------------------
	   wPort=(char)w7000[0];  // RS-232 port number: 1/2/3/4
	   wAddr=w7000[1];	  // module address: 0x00 to 0xFF
	   wID=w7000[2];	  // module ID: 0x7021 or 0x7024
	   wCheckSum=w7000[3];	  // checksum: 0=disable, 1=enable
	   wTimeOut=w7000[4];	  // TimeOut constant: normal=100
	   wReadType=w7000[5];	  //   0: command read back ($AA6)
				  //   1: analog output of current path read back ($AA8)
	   wFlag=(char)w7000[6];  // flag: 0=no save, 1=save send/receive string
	   wChannel=w7000[7];	  //   Channel No.(0 to 3), if wID is 7024
				  //   Not used,	    else
	   //---------------------- output ------------------------------------
				  // f7000[0]=analog output value read back

	/************************************************************/
	/**************** modified function  ************************/
	/************************************************************/
	/*-------- Set configuration for 7080 ---------*/
	EXPORTS WORD CALLBACK SetConfiguration_7080(WORD w7000[], float f7000[],
		char szSendTo7000[], char szReceiveFrom7000[]);
	//---------------------- input -------------------------------------
	//wPort=(char)w7000[0];   // RS-232 port number: 1/2/3/4
	//wAddrOld=w7000[1];	  // module original address: 0x00 to 0xFF
	//wID=w7000[2]; 	  // module ID: 0x7080
	//wCheckSumOld=w7000[3];	  // module original checksum: 0=disable, 1=enable
	//wTimeOut=w7000[4];	  // TimeOut constant: normal=100
	//wFreqGateTime=w7000[5]; // desired frequency gate time:
				  //	  0: 0.1 second
				  //	  1: 1.0 second
	//wFlag=(char)w7000[6];   // flag: 0=no save, 1=save send/receive string
	//wAddrNew=w7000[7];	  // desired new address
	//wType=w7000[8];	  // desired Type->  0:Counter mode
				  //		     1:Frequency mode
	//wBaudrate=w7000[9];	  // desired Baudrate:
				  //	3: 1200 BPS    4:  2400 BPS
				  //	5: 4800 BPS    6:  9600 BPS
				  //	7: 19200 BPS   8:  38400 BPS
				  //	9: 57600 BPS   10: 115200 BPS
	//wCheckSumNew=w7000[10]; // desired Checksum Address

----------------------------------------------------------------------------------------------------------
[Date: July-14, 1998]  [Ver 3.10]

  Remove I7000_ for some function.
----------------------------------------------------------------------------------------------------------
DATE   July, 08, 1998
  I7000_DigitalIn  add the module ID for 7011/7012/7014
----------------------------------------------------------------------------------------------------------
DATE   July, 06, 1998
  Add some command for 7011/7012/7014 to Enable/Disable Alarm
----------------------------------------------------------------------------------------------------------
DATE  June, 15, 1998
  Add the command for 7080/7080D
     (1) set the module mode
	Command:
	   ~AAAM
	Description:
	   M=0	4080  mode
	   M=1	4080D mode
     (2) read the module mode
	Command:
	   ~AAA
	Description
	   !AA0  4080 mode
	   !AA1  4080D mode
----------------------------------------------------------------------------------------------------------
DATE  May, 18, 1998
  Add the I7000_AnalogInHex (reading data in hexadecimal format)
  Add the I7000_AnalogInFsr (reading data in %FSR)

----------------------------------------------------------------------------------------------------------
DATE  April, 28, 1998
  Add the 7080 module in 0204 folder












